Neonode zForce(TM) SDK

- Main Page
- Modules
- Classes
- Files

- Class List
- Class Index
- Class Members

Public Attributes | List of all members
EnableMessage Struct Reference

This structure represents an enable message. More...

`#include <EnableMessage.h>`

## Public Attributes
| Message
| Base Message.
bool | Enabled
| Is Device Enabled.
bool | ContinuousMode
| Is Device set to Continuous Mode.
uint32_t | NumberOfMessages
| Number Of Messages.

## Detailed Description

This structure represents an enable message.

This structure represents a message which indicates if the scanning on a device is turned on and if it is continous or has a defined number of messages to send set.

The documentation for this struct was generated from the following file:

- EnableMessage.h